**Manual switch for three-phase mains disconnection and switching to backup mode**

Manual three-phase mains changeover switch for the PLENTICORE G3 series inverters, integrated cable break detection for the evaluation signal of the switch position, compact and space-saving installation with 8TE, installation in existing sub-distribution board or in separate housing possible, one output each for loads in backup mode and in mains operation, suitable for 3-phase house connections up to 63A, connection of a local neutral point replica possible.

Manufacturer/Type

'Kostal / BackUp-Switch'

or equivalent.

Manufacturer/Type

'....................................................'

to be entered by the bidder.