**1-phase energy meter for measuring the power drawn from and fed into the grid**

Energy meter, for measuring reference and feed-in power at the grid connection point, single-phase measuring mechanism, transmission of domestic consumption or grid feed-in to the connected PLENTICORE series inverter, preconfigured RS485 interfaces, for mounting on top-hat rail, width max. 1 TE, RS485 interface, with active and reactive power measurement, apparent power measurement, current measurement min. 63A, power factor measurement

Manufacturer/Type

'Kostal / KOSTAL Energy Meter MP (type KEM MP-P)'

or equivalent.

Manufacturer/Type

'....................................................'

to be entered by the bidder.