**3-phase energy meter for measuring the power drawn from and fed into the grid**

Energy measuring device, for measuring reference and feed-in power at the grid connection point, 3-phase measuring unit, transmission of domestic consumption or grid feed-in to the connected inverter of the PLENTICORE series, preconfigured RS485 interfaces, for mounting on top-hat rail, width max. 4 HP, RS485 interface, with active and reactive power measurement, apparent power measurement, current measurement min. 63A, power factor measurement per phase

Manufacturer/Type

'Kostal / KOSTAL Energy Meter (type KEM-C or KEM-P)'

or equivalent.

Manufacturer/Type

'....................................................'

to be entered by the bidder.